**Benjamin Moore Regal Select (BM-RS)**

Exhale (pale blue) AF 515

Pashmina (taupe) AF 100

Jute (tan) AF 80

Oklahoma Wheat 2160-50

White Dove OC-17

NOTE

ALL TRIM, DOORS and CROWN (Foyer)
 a) same color as wall EXCEPT front door, see below (k, L, m)

 b) semi-gloss latex

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Surface** | **Location** | **Color** | **Type** | **NOTES** |
|  |  | Exhale (pale blue) | Pashmina (taupe) | Jute (tan) | Oklahoma Wheat | White Dove | Flat | Semi-Gloss |  |
| ceilings | ceilings |  |  |  |  | X | F |  |  |
| a | kitchen/nook left (north)=long wall | X |  |  |  |  | F |  |  |
| b | nook back (east) |  |  | X |  |  | F |  |  |
| c | nook right (south) |  |  | X |  |  | F |  |  |
| d | back wall (east) |  |  | X |  |  | F |  |  |
| e | fireplace wall  |  | X |  |  |  | F |  |  |
| f | fm rm divider |  | X |  |  |  | F |  |  |
| g | middle r m divider |  | X |  |  |  | F |  |  |
| h | middle r m windows |  | X |  |  |  | F |  |  |
| i | middle r m entrance |  | X |  |  |  | F |  |  |
| j | entrance divider |  |  | X |  |  | F |  |  |
| k | FRONT door **wall** |  |  | X |  |  | F |  |  |
| L | FRONT **door** | **X** |  |  |  |  |  | S |  |
| m | FRONTfront door **trim** |  |  |  |  | **X** |  | S |  |
| n | "foyer" entrance top joist |  |  | X |  |  | F |  |  |
| o | foyer walls TOP |  |  | X |  |  | F |  |  |
| p | foyer walls BOTTOM |  | X |  |  |  | F |  |  |
| q | foyer walls CHAIR RAIL |  |  |  |  | X |  | S |  |
| aa | foyer DOORS ALL except front  |  |  | X |  |  |  | S |  |
| r | closet wall |  |  | X |  |  | F |  |  |
| s | closet INSIDE | X |  |  |  |  | F |  |  |
| t | hallway left (west) |  |  | X |  |  | F |  |  |
| u | hallway back (north) | X |  |  |  |  | F |  |  |
| v | hallway right (kitchen) |  |  | X |  |  | F |  |  |
| w | laundry left (south) |  |  |  | X |  | F |  |  |
| x | laundry door (west) |  |  |  | X |  | F |  |  |
| y | laundry right (north) |  |  |  | X |  | F |  |  |
| z | laundry back (east) |  |  |  | X |  | F |  |  |